1. Move lumbar support adjustment all the way back.

2. Unclip the two locking lugs **-1-** on the rear seat by pressing them with a screwdriver.

3. Lift the rear seat up slightly **-arrow A-** and release and disconnect the electric plug connection

**-arrow B-**

